source ~/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/ENV/bin/activate

python ~/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/GRWatch/trinket.py

(ENV)pjloury@PJnet: ~/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/GRWatch $ python ~/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/GRWatch/trinket.py

Begin Control Session...

reading

?

1?1

1

1

^[[A^[[B1

3

1

?L?????L?L?H?1

1

1

1

1

1

1

1

Traceback (most recent call last):

File "/Users/pjloury/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/GRWatch/trinket.py", line 95, in <module>

serial\_read()

File "/Users/pjloury/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/GRWatch/trinket.py", line 37, in serial\_read

raw0 = ser.readline()

File "/Users/pjloury/Dropbox/Wristband/Serial\_port\_console\_ian\_v1.0/ENV/lib/python2.7/site-packages/serial/serialposix.py", line 475, in read

raise SerialException('device reports readiness to read but returned no data (device disconnected or multiple access on port?)')

serial.serialutil.SerialException: device reports readiness to read but returned no data (device disconnected or multiple access on port?)